HDMI jack RRJ(VA)\_HDMI(\_SW)

|  |  |  |  |
| --- | --- | --- | --- |
| \\A013\Wer\Fotos\Befehlsgeraete\Baureihe RONTRON-R-JUWEL\RRJ_HDMI.jpg | \\A013\Wer\Fotos\Befehlsgeraete\Baureihe RONTRON-R-JUWEL\RRJVA_HDMI.jpg | \\A013\Wer\Fotos\Befehlsgeraete\Baureihe RONTRON-R-JUWEL\RRJ_HDMI_SW.jpg | \\A013\Wer\Fotos\Befehlsgeraete\Baureihe RONTRON-R-JUWEL\RRJ_HDMI_m.png |
| RRJ\_HDMI | RRJVA\_HDMI | RRJ\_HDMI\_SW |  |

Overview

HDMI jack with HDMI connector and 60 cm cable.

Technical data

|  |  |  |  |
| --- | --- | --- | --- |
| RRJ\_HDMI | RRJVA\_HDMI | | RRJ\_HDMI\_SW |
| Panel cut-out  Front: USB-C jack  Rear: connector  Cable length (X)  Rated voltage  Rated current  Storage temperature  Operating temperature  Mechanical life | | Ø 22,3 mm  HDMI 1.4 jack  HDMI 1.4 connector  60 cm + 3 cm  max. 40 V  max. 0.5 A  -25°C ... 60°C  -25°C ... 60°C  5,000 mating cycles | |
| [Data sheet](https://www.schlegel.biz/web/de/produktkonfigurator/RONTRON-R-JUWEL/RRJ_HDMI|HDMI-Buchse+Stecker/pdf-datenblatt.pdf) | [Data sheet](https://www.schlegel.biz/web/de/produktkonfigurator/RONTRON-R-JUWEL/RRJVA_HDMI|HDMI-Buchse+Stecker/pdf-datenblatt.pdf) | | [Data sheet](https://www.schlegel.biz/web/de/produktkonfigurator/RONTRON-R-JUWEL/RRJ_HDMI_SW|HDMI-Buchse+Stecker/pdf-datenblatt.pdf) |

[Dates, prices and order data](#Typenliste)

* Product availability

From now on (samples are available upon request)

* Delivery time

Standard

* Price list with order data

|  |  |  |
| --- | --- | --- |
| RRJ\_HDMI | RRJVA\_HDMI | RRJ\_HDMI\_SW |
| 35.05 € | 48.68 € | 33.51 € |

Date\*: 07/2021

\* The price information is not binding and may finally differ slightly.